**Freifunk Mesh**

* *Universal Settings*
  + Admin Username: root
  + Admin Password: grizzly
  + ESSID: Kansas
  + BSSID: 02:CA:FF:EE:KA:BE
  + Multicast Rate: 5.5mbps/Auto
  + HNA4: 192.168.2.0/24
  + Disable Firewall
  + Permit SSH
  + Permit HTTP
  + Permit HTTPS
  + Permit Ping
* *Gateway Router*
  + Wireless: 192.168.2.1
  + LAN: 192.168.3.1
* *North Router*
  + Wireless: 192.168.2.2
  + LAN: 192.168.4.1
* *Creek Router*
  + Wireless: 192.168.2.3
  + LAN: 192.168.5.1
* *South Router*
  + Wireless: 192.168.2.4
  + LAN: 192.168.6.1
* *Relay Router*
  + Wireless: 192.168.2.5
  + LAN: 192.168.7.1
* *Well 2 Router*
  + Wireless: 192.168.2.6
  + LAN: 192.168.8.1
* *Extra Router*
  + Wireless: 192.168.2.7
  + LAN: 192.168.9.1

**Tomato Access Points**

* *Universal Settings*
  + Admin Username: admin
  + Admin Password: grizzly
  + Wireless Node: Access Point
  + Security: WPA-Personal
  + Encryption: TKIP
  + Shared Key: kansasapgrizzly
* *Gateway AP*
  + SSID: Gateway AP
  + LAN: 192.168.15.1
* *North AP*
  + SSID: North AP
  + LAN: 192.168.14.1
* *Creek AP*
  + SSID: Creek AP
  + LAN: 192.168.11.1
* *South AP*
  + SSID: South AP
  + LAN: 192.168.13.1
* *Relay AP*
  + SSID: Relay AP
  + LAN: 192.168.12.1
* *Well 2 AP*
  + SSID: Well 2 AP
  + LAN: 192.168.15.1

**IP Cameras**

* *Universal Settings*
  + Admin Username: admin
  + Admin Password: grizzly
* *Gateway Cam*
  + ID: 003afnd
  + IP: 192.168.15.99
  + Gateway/DNS: 192.168.15.1
* *North Cam*
  + ID: 003agnr
  + IP: 192.168.14.99
  + Gateway/DNS: 192.168.14.1
* *Creek Cam*
  + ID: 003afmf
  + IP: 192.168.11.99
  + Gateway/DNS: 192.168.11.1
* *South Cam*
  + ID: 003afnb
  + IP: 192.168.13.99
  + Gateway/DNS: 192.168.13.1
* *Relay Cam*
  + ID: 003afnf
  + IP: 192.168.12.99
  + Gateway/DNS: 192.168.12.1
* *Well 2 Cam*
  + ID: 003afov
  + IP: 192.168.10.99
  + Gateway/DNS: 192.168.10.1